<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="58.41" width="0" layer="20"/>
<wire x1="100" y1="58.41" x2="0" y2="58.41" width="0" layer="20"/>
<wire x1="0" y1="58.41" x2="0" y2="0" width="0" layer="20"/>
<text>Coté Cuivre</text>
<text>Coté Cuivre</text>
<text>Coté Cuivre</text>
<text>Coté Cuivre</text>
<text>DMX 1.1</text>
</plain>
<libraries>
<library name="751xx">
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="optocoupler">
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="resistor">
<packages>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="0207/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 12 mm</description>
</package>
<package name="E2,5-7">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 7 mm</description>
</package>
<package name="C025-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.4 x 4.4 mm</description>
</package>
</packages>
</library>
<library name="diode">
<packages>
<package name="DO35-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2 mm, horizontal, grid 10.16 mm</description>
</package>
</packages>
</library>
<library name="v-reg">
<packages>
<package name="78XXL">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-phoenix-254">
<packages>
<package name="3POL254">
<description>&lt;b&gt;PHOENIX CONNECTOR&lt;/b&gt;</description>
</package>
<package name="8POL254">
<description>&lt;b&gt;PHOENIX CONNECTOR&lt;/b&gt;</description>
</package>
<package name="9POL254">
<description>&lt;b&gt;PHOENIX CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="arduino">
<packages>
<package name="MEGA_ARDUINO_2">
</package>
</packages>
</library>
<library name="trafo">
<description>&lt;b&gt;Transformers&lt;/b&gt;&lt;p&gt;
Based on the following previous libraries:
&lt;ul&gt;
&lt;li&gt;trafo-b.lbr: transformers from BLOCK
&lt;li&gt;trafo-e.lbr: transformers from ERA
&lt;li&gt;trafo-r.lbr: ring cores
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="VR07,5-2">
<description>&lt;b&gt;TRANSFORMER&lt;/b&gt;&lt;p&gt;
1 primary winding, 2 secondary windings, mounting holes</description>
</package>
</packages>
</library>
<library name="fuse">
<description>&lt;b&gt;Fuses and Fuse Holders&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SH22,5">
<description>&lt;b&gt;FUSE HOLDER&lt;/b&gt;&lt;p&gt; grid 22,5 mm, OGN0031 8201 Schurter (Buerklin)</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="751xx" package="DIL08" value="75176AP"/>
<element name="IC2" library="751xx" package="DIL08" value="75176AP"/>
<element name="OK1" library="optocoupler" package="DIL08" value="HCPL2630">
<attribute name="MF" value="AGILENT TECHNOLOGIES"/>
<attribute name="MPN" value="HCPL-2630-000E"/>
<attribute name="OC_FARNELL" value="9994904"/>
<attribute name="OC_NEWARK" value="88H7813"/>
</element>
<element name="R1" library="resistor" package="0207/12" value="120"/>
<element name="R2" library="resistor" package="0207/12" value="470"/>
<element name="R3" library="resistor" package="0207/12" value="120"/>
<element name="R4" library="resistor" package="0207/12" value="120"/>
<element name="R5" library="resistor" package="0207/12" value="120"/>
<element name="D1" library="diode" package="DO35-10" value="1N4148DO35-10"/>
<element name="D2" library="diode" package="DO35-10" value="1N4148DO35-10"/>
<element name="D3" library="diode" package="DO35-10" value="1N4148DO35-10"/>
<element name="D4" library="diode" package="DO35-10" value="1N4148DO35-10"/>
<element name="C1" library="resistor" package="E2,5-7" value=""/>
<element name="IC3" library="v-reg" package="78XXL" value=""/>
<element name="OK2" library="optocoupler" package="DIL08" value="HCPL2630">
<attribute name="MF" value="AGILENT TECHNOLOGIES"/>
<attribute name="MPN" value="HCPL-2630-000E"/>
<attribute name="OC_FARNELL" value="9994904"/>
<attribute name="OC_NEWARK" value="88H7813"/>
</element>
<element name="R6" library="resistor" package="0207/12" value="470"/>
<element name="DMX-T" library="con-phoenix-254" package="3POL254" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="DMX-R" library="con-phoenix-254" package="3POL254" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="C2" library="resistor" package="C025-024X044" value=""/>
<element name="IC4" library="arduino" package="MEGA_ARDUINO_2" value=""/>
<element name="ANAL1" library="con-phoenix-254" package="8POL254" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="ANAL2" library="con-phoenix-254" package="8POL254" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="X1" library="con-phoenix-254" package="8POL254" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="X2" library="con-phoenix-254" package="8POL254" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="R7" library="resistor" package="0204/7" value=""/>
<element name="R8" library="resistor" package="0204/7" value=""/>
<element name="R9" library="resistor" package="0204/7" value=""/>
<element name="R10" library="resistor" package="0204/7" value=""/>
<element name="R11" library="resistor" package="0204/7" value=""/>
<element name="R12" library="resistor" package="0204/7" value=""/>
<element name="R13" library="resistor" package="0204/7" value=""/>
<element name="R14" library="resistor" package="0204/7" value=""/>
<element name="R15" library="resistor" package="0204/7" value=""/>
<element name="R16" library="resistor" package="0204/7" value=""/>
<element name="R17" library="resistor" package="0204/7" value=""/>
<element name="R18" library="resistor" package="0204/7" value=""/>
<element name="R19" library="resistor" package="0204/7" value=""/>
<element name="R20" library="resistor" package="0204/7" value=""/>
<element name="L1" library="con-phoenix-254" package="9POL254" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="L2" library="con-phoenix-254" package="9POL254" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="L3" library="con-phoenix-254" package="9POL254" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="L4" library="con-phoenix-254" package="9POL254" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="TR1" library="trafo" package="VR07,5-2" value=""/>
<element name="D5" library="diode" package="DO35-10" value="1N4148DO35-10"/>
<element name="D6" library="diode" package="DO35-10" value="1N4148DO35-10"/>
<element name="D7" library="diode" package="DO35-10" value="1N4148DO35-10"/>
<element name="D8" library="diode" package="DO35-10" value="1N4148DO35-10"/>
<element name="C3" library="resistor" package="E2,5-7" value=""/>
<element name="IC5" library="751xx" package="DIL08" value="75176AP"/>
<element name="OK3" library="optocoupler" package="DIL08" value="HCPL2630">
<attribute name="OC_NEWARK" value="88H7813"/>
<attribute name="MPN" value="HCPL-2630-000E"/>
<attribute name="MF" value="AGILENT TECHNOLOGIES"/>
<attribute name="OC_FARNELL" value="9994904"/>
</element>
<element name="R21" library="resistor" package="0207/12" value="120"/>
<element name="R22" library="resistor" package="0207/12" value="470"/>
<element name="R23" library="resistor" package="0207/12" value="120"/>
<element name="DMX-T1" library="con-phoenix-254" package="3POL254" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="F1" library="fuse" package="SH22,5" value="">
<attribute name="OC_NEWARK" value="96F8317"/>
<attribute name="MPN" value="0031.8201"/>
<attribute name="MF" value="SCHURTER"/>
<attribute name="OC_FARNELL" value="1162740"/>
</element>
<element name="AC-1" library="con-phoenix-254" package="3POL254" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
</elements>
<signals>
<signal name="+3V3">
<contactref element="IC4" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="D1" pad="C"/>
<contactref element="D2" pad="A"/>
<contactref element="TR1" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="D3" pad="C"/>
<contactref element="D4" pad="A"/>
<contactref element="TR1" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="D2" pad="C"/>
<contactref element="D4" pad="C"/>
<contactref element="C1" pad="+"/>
<contactref element="IC3" pad="IN"/>
</signal>
<signal name="N$6">
<contactref element="R1" pad="2"/>
<contactref element="OK1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="6"/>
<contactref element="R3" pad="2"/>
<contactref element="DMX-T" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="7"/>
<contactref element="R3" pad="1"/>
<contactref element="DMX-T" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="R1" pad="1"/>
<contactref element="IC4" pad="26"/>
</signal>
<signal name="N$13">
<contactref element="IC2" pad="6"/>
<contactref element="R4" pad="2"/>
<contactref element="DMX-R" pad="3"/>
</signal>
<signal name="N$14">
<contactref element="IC2" pad="7"/>
<contactref element="R4" pad="1"/>
<contactref element="DMX-R" pad="2"/>
</signal>
<signal name="GND">
<contactref element="OK1" pad="5"/>
<contactref element="IC1" pad="5"/>
<contactref element="DMX-T" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="D3" pad="A"/>
<contactref element="C1" pad="-"/>
<contactref element="IC3" pad="GND"/>
<contactref element="C2" pad="2"/>
<contactref element="IC2" pad="2"/>
<contactref element="IC2" pad="3"/>
<contactref element="IC2" pad="4"/>
<contactref element="OK2" pad="2"/>
<contactref element="IC2" pad="5"/>
<contactref element="DMX-R" pad="1"/>
<contactref element="IC5" pad="5"/>
<contactref element="OK3" pad="5"/>
<contactref element="IC5" pad="5"/>
<contactref element="DMX-T1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="8"/>
<contactref element="IC3" pad="OUT"/>
<contactref element="C2" pad="1"/>
<contactref element="IC2" pad="8"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="OK1" pad="8"/>
<contactref element="IC5" pad="8"/>
<contactref element="IC5" pad="8"/>
<contactref element="IC5" pad="3"/>
<contactref element="IC5" pad="2"/>
<contactref element="R22" pad="2"/>
<contactref element="OK3" pad="8"/>
</signal>
<signal name="N$4">
<contactref element="R5" pad="2"/>
<contactref element="OK2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="IC2" pad="1"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$32">
<contactref element="OK2" pad="7"/>
<contactref element="R6" pad="1"/>
<contactref element="IC4" pad="25"/>
</signal>
<signal name="N$15">
<contactref element="OK2" pad="8"/>
<contactref element="R6" pad="2"/>
<contactref element="IC4" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="IC4" pad="7"/>
<contactref element="ANAL1" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC4" pad="22"/>
<contactref element="ANAL2" pad="8"/>
</signal>
<signal name="N$9">
<contactref element="IC4" pad="21"/>
<contactref element="ANAL2" pad="7"/>
</signal>
<signal name="N$16">
<contactref element="IC4" pad="20"/>
<contactref element="ANAL2" pad="6"/>
</signal>
<signal name="N$17">
<contactref element="IC4" pad="19"/>
<contactref element="ANAL2" pad="5"/>
</signal>
<signal name="N$18">
<contactref element="IC4" pad="18"/>
<contactref element="ANAL2" pad="4"/>
</signal>
<signal name="N$19">
<contactref element="IC4" pad="17"/>
<contactref element="ANAL2" pad="3"/>
</signal>
<signal name="N$20">
<contactref element="IC4" pad="16"/>
<contactref element="ANAL2" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="IC4" pad="15"/>
<contactref element="ANAL2" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="IC4" pad="14"/>
<contactref element="ANAL1" pad="8"/>
</signal>
<signal name="N$23">
<contactref element="IC4" pad="13"/>
<contactref element="ANAL1" pad="7"/>
</signal>
<signal name="N$24">
<contactref element="IC4" pad="12"/>
<contactref element="ANAL1" pad="6"/>
</signal>
<signal name="N$25">
<contactref element="IC4" pad="11"/>
<contactref element="ANAL1" pad="5"/>
</signal>
<signal name="N$26">
<contactref element="IC4" pad="10"/>
<contactref element="ANAL1" pad="4"/>
</signal>
<signal name="N$27">
<contactref element="IC4" pad="9"/>
<contactref element="ANAL1" pad="3"/>
</signal>
<signal name="N$28">
<contactref element="IC4" pad="8"/>
<contactref element="ANAL1" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="IC4" pad="37"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$31">
<contactref element="IC4" pad="38"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$33">
<contactref element="IC4" pad="35"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$34">
<contactref element="IC4" pad="36"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="IC4" pad="33"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$36">
<contactref element="IC4" pad="34"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$37">
<contactref element="IC4" pad="31"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$38">
<contactref element="IC4" pad="32"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$39">
<contactref element="IC4" pad="46"/>
<contactref element="X2" pad="8"/>
</signal>
<signal name="N$41">
<contactref element="IC4" pad="39"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="N$42">
<contactref element="IC4" pad="40"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="N$43">
<contactref element="IC4" pad="41"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="N$44">
<contactref element="IC4" pad="42"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="N$45">
<contactref element="IC4" pad="43"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="N$46">
<contactref element="IC4" pad="44"/>
<contactref element="R20" pad="1"/>
</signal>
<signal name="N$47">
<contactref element="R7" pad="1"/>
<contactref element="X1" pad="7"/>
</signal>
<signal name="N$48">
<contactref element="R8" pad="1"/>
<contactref element="X1" pad="8"/>
</signal>
<signal name="N$49">
<contactref element="R15" pad="1"/>
<contactref element="X2" pad="1"/>
</signal>
<signal name="N$50">
<contactref element="R16" pad="1"/>
<contactref element="X2" pad="2"/>
</signal>
<signal name="N$51">
<contactref element="R17" pad="2"/>
<contactref element="X2" pad="3"/>
</signal>
<signal name="N$52">
<contactref element="R18" pad="2"/>
<contactref element="X2" pad="4"/>
</signal>
<signal name="N$53">
<contactref element="R19" pad="2"/>
<contactref element="X2" pad="5"/>
</signal>
<signal name="N$54">
<contactref element="R20" pad="2"/>
<contactref element="X2" pad="6"/>
</signal>
<signal name="N$55">
<contactref element="R13" pad="2"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="N$56">
<contactref element="R14" pad="2"/>
<contactref element="X1" pad="2"/>
</signal>
<signal name="N$57">
<contactref element="R10" pad="2"/>
<contactref element="X1" pad="6"/>
</signal>
<signal name="N$58">
<contactref element="R11" pad="2"/>
<contactref element="X1" pad="3"/>
</signal>
<signal name="N$59">
<contactref element="R12" pad="2"/>
<contactref element="X1" pad="4"/>
</signal>
<signal name="N$60">
<contactref element="IC4" pad="47"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="N$61">
<contactref element="IC4" pad="49"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="N$62">
<contactref element="IC4" pad="51"/>
<contactref element="L1" pad="3"/>
</signal>
<signal name="N$65">
<contactref element="IC4" pad="57"/>
<contactref element="L1" pad="6"/>
</signal>
<signal name="N$66">
<contactref element="IC4" pad="59"/>
<contactref element="L1" pad="7"/>
</signal>
<signal name="N$67">
<contactref element="IC4" pad="61"/>
<contactref element="L1" pad="8"/>
</signal>
<signal name="N$68">
<contactref element="IC4" pad="63"/>
<contactref element="L1" pad="9"/>
</signal>
<signal name="N$69">
<contactref element="IC4" pad="65"/>
<contactref element="L2" pad="1"/>
</signal>
<signal name="N$70">
<contactref element="IC4" pad="67"/>
<contactref element="L2" pad="2"/>
</signal>
<signal name="N$71">
<contactref element="IC4" pad="69"/>
<contactref element="L2" pad="3"/>
</signal>
<signal name="N$72">
<contactref element="IC4" pad="71"/>
<contactref element="L2" pad="4"/>
</signal>
<signal name="N$73">
<contactref element="IC4" pad="73"/>
<contactref element="L2" pad="5"/>
</signal>
<signal name="N$74">
<contactref element="IC4" pad="75"/>
<contactref element="L2" pad="6"/>
</signal>
<signal name="N$75">
<contactref element="IC4" pad="77"/>
<contactref element="L2" pad="7"/>
</signal>
<signal name="N$76">
<contactref element="IC4" pad="79"/>
<contactref element="L2" pad="8"/>
</signal>
<signal name="N$77">
<contactref element="IC4" pad="81"/>
<contactref element="L2" pad="9"/>
</signal>
<signal name="N$78">
<contactref element="IC4" pad="48"/>
<contactref element="L3" pad="1"/>
</signal>
<signal name="N$79">
<contactref element="IC4" pad="50"/>
<contactref element="L3" pad="2"/>
</signal>
<signal name="N$80">
<contactref element="IC4" pad="52"/>
<contactref element="L3" pad="3"/>
</signal>
<signal name="N$81">
<contactref element="IC4" pad="54"/>
<contactref element="L3" pad="4"/>
</signal>
<signal name="N$82">
<contactref element="IC4" pad="56"/>
<contactref element="L3" pad="5"/>
</signal>
<signal name="N$83">
<contactref element="IC4" pad="58"/>
<contactref element="L3" pad="6"/>
</signal>
<signal name="N$84">
<contactref element="IC4" pad="60"/>
<contactref element="L3" pad="7"/>
</signal>
<signal name="N$85">
<contactref element="IC4" pad="62"/>
<contactref element="L3" pad="8"/>
</signal>
<signal name="N$86">
<contactref element="IC4" pad="64"/>
<contactref element="L3" pad="9"/>
</signal>
<signal name="N$87">
<contactref element="IC4" pad="66"/>
<contactref element="L4" pad="1"/>
</signal>
<signal name="N$88">
<contactref element="IC4" pad="68"/>
<contactref element="L4" pad="2"/>
</signal>
<signal name="N$89">
<contactref element="IC4" pad="70"/>
<contactref element="L4" pad="3"/>
</signal>
<signal name="N$90">
<contactref element="IC4" pad="72"/>
<contactref element="L4" pad="4"/>
</signal>
<signal name="N$91">
<contactref element="IC4" pad="74"/>
<contactref element="L4" pad="5"/>
</signal>
<signal name="N$92">
<contactref element="IC4" pad="76"/>
<contactref element="L4" pad="6"/>
</signal>
<signal name="N$93">
<contactref element="IC4" pad="78"/>
<contactref element="L4" pad="7"/>
</signal>
<signal name="N$94">
<contactref element="IC4" pad="80"/>
<contactref element="L4" pad="8"/>
</signal>
<signal name="N$95">
<contactref element="IC4" pad="82"/>
<contactref element="L4" pad="9"/>
</signal>
<signal name="N$96">
<contactref element="R9" pad="1"/>
<contactref element="X1" pad="5"/>
</signal>
<signal name="N$63">
<contactref element="IC4" pad="53"/>
<contactref element="L1" pad="4"/>
</signal>
<signal name="N$64">
<contactref element="IC4" pad="55"/>
<contactref element="L1" pad="5"/>
</signal>
<signal name="N$97">
<contactref element="IC1" pad="4"/>
<contactref element="R2" pad="1"/>
<contactref element="OK1" pad="7"/>
</signal>
<signal name="N$98">
<contactref element="IC4" pad="45"/>
<contactref element="X2" pad="7"/>
</signal>
<signal name="N$40">
<contactref element="IC4" pad="4"/>
</signal>
<signal name="N$99">
</signal>
<signal name="N$100">
<contactref element="D5" pad="C"/>
<contactref element="D6" pad="A"/>
<contactref element="TR1" pad="6"/>
</signal>
<signal name="N$101">
<contactref element="D7" pad="C"/>
<contactref element="D8" pad="A"/>
<contactref element="TR1" pad="5"/>
</signal>
<signal name="N$102">
<contactref element="D6" pad="C"/>
<contactref element="D8" pad="C"/>
<contactref element="C3" pad="+"/>
<contactref element="IC4" pad="6"/>
</signal>
<signal name="GND1">
<contactref element="D5" pad="A"/>
<contactref element="D7" pad="A"/>
<contactref element="C3" pad="-"/>
<contactref element="OK2" pad="5"/>
<contactref element="OK1" pad="2"/>
<contactref element="IC4" pad="5"/>
<contactref element="OK3" pad="2"/>
</signal>
<signal name="N$104">
<contactref element="R21" pad="2"/>
<contactref element="OK3" pad="1"/>
</signal>
<signal name="N$105">
<contactref element="IC5" pad="6"/>
<contactref element="R23" pad="2"/>
<contactref element="DMX-T1" pad="3"/>
</signal>
<signal name="N$106">
<contactref element="IC5" pad="7"/>
<contactref element="R23" pad="1"/>
<contactref element="DMX-T1" pad="2"/>
</signal>
<signal name="N$107">
<contactref element="R21" pad="1"/>
<contactref element="IC4" pad="28"/>
</signal>
<signal name="N$108">
<contactref element="IC5" pad="4"/>
<contactref element="R22" pad="1"/>
<contactref element="OK3" pad="7"/>
</signal>
<signal name="N$110">
<contactref element="F1" pad="2"/>
<contactref element="TR1" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="AC-1" pad="1"/>
<contactref element="F1" pad="1"/>
</signal>
<signal name="N$103">
<contactref element="AC-1" pad="2"/>
<contactref element="TR1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
