<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<text>Coté Cuivre</text>
<hole x="-15.24" y="64.77" drill="0.6"/>
<hole x="248.92" y="64.77" drill="0.6"/>
<hole x="248.92" y="-44.45" drill="0.6"/>
<hole x="-15.24" y="-44.45" drill="0.6"/>
<hole x="-58.42" y="-7.62" drill="0.6"/>
<hole x="-300.99" y="-7.62" drill="0.6"/>
<hole x="-300.99" y="-34.29" drill="0.6"/>
<hole x="-58.42" y="-34.29" drill="0.6"/>
<hole x="-121.92" y="62.23" drill="0.6"/>
<hole x="-121.92" y="11.43" drill="0.6"/>
<hole x="-175.26" y="11.43" drill="0.6"/>
<hole x="-173.99" y="62.23" drill="0.6"/>
</plain>
<libraries>
<library name="751xx">
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="optocoupler">
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="resistor">
<packages>
<package name="0207/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 12 mm</description>
</package>
<package name="E2,5-7">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 7 mm</description>
</package>
<package name="C025-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.4 x 4.4 mm</description>
</package>
</packages>
</library>
<library name="diode">
<packages>
<package name="DO35-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2 mm, horizontal, grid 10.16 mm</description>
</package>
</packages>
</library>
<library name="v-reg">
<packages>
<package name="78XXL">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-phoenix-254">
<packages>
<package name="3POL254">
<description>&lt;b&gt;PHOENIX CONNECTOR&lt;/b&gt;</description>
</package>
<package name="2POL254">
<description>&lt;b&gt;PHOENIX CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="arduino">
<packages>
<package name="MEGA_ARDUINO_2">
</package>
</packages>
</library>
<library name="trafo">
<description>&lt;b&gt;Transformers&lt;/b&gt;&lt;p&gt;
Based on the following previous libraries:
&lt;ul&gt;
&lt;li&gt;trafo-b.lbr: transformers from BLOCK
&lt;li&gt;trafo-e.lbr: transformers from ERA
&lt;li&gt;trafo-r.lbr: ring cores
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="VR07,5-2">
<description>&lt;b&gt;TRANSFORMER&lt;/b&gt;&lt;p&gt;
1 primary winding, 2 secondary windings, mounting holes</description>
</package>
</packages>
</library>
<library name="fuse">
<description>&lt;b&gt;Fuses and Fuse Holders&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SH22,5">
<description>&lt;b&gt;FUSE HOLDER&lt;/b&gt;&lt;p&gt; grid 22,5 mm, OGN0031 8201 Schurter (Buerklin)</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="perso">
<packages>
<package name="POT-LIN-BOURNS">
</package>
</packages>
</library>
<library name="con-harting-v">
<description>&lt;b&gt;Harting Connectors&lt;/b&gt;&lt;p&gt;
PC board mounted ribbon cable connectors (IEC 52141), vertical&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="40V">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="751xx" package="DIL08" value="75176AP"/>
<element name="IC2" library="751xx" package="DIL08" value="75176AP"/>
<element name="OK1" library="optocoupler" package="DIL08" value="HCPL2630">
<attribute name="MF" value="AGILENT TECHNOLOGIES"/>
<attribute name="MPN" value="HCPL-2630-000E"/>
<attribute name="OC_FARNELL" value="9994904"/>
<attribute name="OC_NEWARK" value="88H7813"/>
</element>
<element name="R1" library="resistor" package="0207/12" value="120"/>
<element name="R2" library="resistor" package="0207/12" value="470"/>
<element name="R3" library="resistor" package="0207/12" value="120"/>
<element name="R4" library="resistor" package="0207/12" value="120"/>
<element name="R5" library="resistor" package="0207/12" value="120"/>
<element name="D1" library="diode" package="DO35-10" value="1N4148DO35-10"/>
<element name="D2" library="diode" package="DO35-10" value="1N4148DO35-10"/>
<element name="D3" library="diode" package="DO35-10" value="1N4148DO35-10"/>
<element name="D4" library="diode" package="DO35-10" value="1N4148DO35-10"/>
<element name="C1" library="resistor" package="E2,5-7" value=""/>
<element name="IC3" library="v-reg" package="78XXL" value=""/>
<element name="OK2" library="optocoupler" package="DIL08" value="HCPL2630">
<attribute name="MF" value="AGILENT TECHNOLOGIES"/>
<attribute name="MPN" value="HCPL-2630-000E"/>
<attribute name="OC_FARNELL" value="9994904"/>
<attribute name="OC_NEWARK" value="88H7813"/>
</element>
<element name="R6" library="resistor" package="0207/12" value="470"/>
<element name="DMX-T" library="con-phoenix-254" package="3POL254" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="DMX-R" library="con-phoenix-254" package="3POL254" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="C2" library="resistor" package="C025-024X044" value=""/>
<element name="IC4" library="arduino" package="MEGA_ARDUINO_2" value=""/>
<element name="TR1" library="trafo" package="VR07,5-2" value=""/>
<element name="D5" library="diode" package="DO35-10" value="1N4148DO35-10"/>
<element name="D6" library="diode" package="DO35-10" value="1N4148DO35-10"/>
<element name="D7" library="diode" package="DO35-10" value="1N4148DO35-10"/>
<element name="D8" library="diode" package="DO35-10" value="1N4148DO35-10"/>
<element name="C3" library="resistor" package="E2,5-7" value=""/>
<element name="IC5" library="751xx" package="DIL08" value="75176AP"/>
<element name="OK3" library="optocoupler" package="DIL08" value="HCPL2630">
<attribute name="OC_NEWARK" value="88H7813"/>
<attribute name="MPN" value="HCPL-2630-000E"/>
<attribute name="MF" value="AGILENT TECHNOLOGIES"/>
<attribute name="OC_FARNELL" value="9994904"/>
</element>
<element name="R21" library="resistor" package="0207/12" value="120"/>
<element name="R22" library="resistor" package="0207/12" value="470"/>
<element name="R23" library="resistor" package="0207/12" value="120"/>
<element name="DMX-T1" library="con-phoenix-254" package="3POL254" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="F1" library="fuse" package="SH22,5" value="">
<attribute name="OC_NEWARK" value="96F8317"/>
<attribute name="MPN" value="0031.8201"/>
<attribute name="MF" value="SCHURTER"/>
<attribute name="OC_FARNELL" value="1162740"/>
</element>
<element name="AC-1" library="con-phoenix-254" package="3POL254" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="R7" library="resistor" package="0207/12" value="1000"/>
<element name="LED1" library="led" package="LED3MM" value=""/>
<element name="R8" library="resistor" package="0207/12" value="1000"/>
<element name="LED2" library="led" package="LED3MM" value=""/>
<element name="R9" library="resistor" package="0207/12" value="1000"/>
<element name="LED3" library="led" package="LED3MM" value=""/>
<element name="R10" library="resistor" package="0207/12" value="120"/>
<element name="C4" library="resistor" package="C025-024X044" value=""/>
<element name="X1" library="con-phoenix-254" package="2POL254" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="R11" library="resistor" package="0207/12" value="0"/>
<element name="P1" library="perso" package="POT-LIN-BOURNS" value="POT-LIN-BOURNS"/>
<element name="R12" library="resistor" package="0207/12" value="0"/>
<element name="P2" library="perso" package="POT-LIN-BOURNS" value="POT-LIN-BOURNS"/>
<element name="R13" library="resistor" package="0207/12" value="0"/>
<element name="P3" library="perso" package="POT-LIN-BOURNS" value="POT-LIN-BOURNS"/>
<element name="R14" library="resistor" package="0207/12" value="0"/>
<element name="P4" library="perso" package="POT-LIN-BOURNS" value="POT-LIN-BOURNS"/>
<element name="R15" library="resistor" package="0207/12" value="0"/>
<element name="P5" library="perso" package="POT-LIN-BOURNS" value="POT-LIN-BOURNS"/>
<element name="R16" library="resistor" package="0207/12" value="0"/>
<element name="P6" library="perso" package="POT-LIN-BOURNS" value="POT-LIN-BOURNS"/>
<element name="R17" library="resistor" package="0207/12" value="0"/>
<element name="P7" library="perso" package="POT-LIN-BOURNS" value="POT-LIN-BOURNS"/>
<element name="R18" library="resistor" package="0207/12" value="0"/>
<element name="P8" library="perso" package="POT-LIN-BOURNS" value="POT-LIN-BOURNS"/>
<element name="R19" library="resistor" package="0207/12" value="0"/>
<element name="P9" library="perso" package="POT-LIN-BOURNS" value="POT-LIN-BOURNS"/>
<element name="R20" library="resistor" package="0207/12" value="0"/>
<element name="P10" library="perso" package="POT-LIN-BOURNS" value="POT-LIN-BOURNS"/>
<element name="R24" library="resistor" package="0207/12" value="0"/>
<element name="P11" library="perso" package="POT-LIN-BOURNS" value="POT-LIN-BOURNS"/>
<element name="R25" library="resistor" package="0207/12" value="0"/>
<element name="P12" library="perso" package="POT-LIN-BOURNS" value="POT-LIN-BOURNS"/>
<element name="R26" library="resistor" package="0207/12" value="0"/>
<element name="P13" library="perso" package="POT-LIN-BOURNS" value="POT-LIN-BOURNS"/>
<element name="R27" library="resistor" package="0207/12" value="0"/>
<element name="P14" library="perso" package="POT-LIN-BOURNS" value="POT-LIN-BOURNS"/>
<element name="R28" library="resistor" package="0207/12" value="0"/>
<element name="P15" library="perso" package="POT-LIN-BOURNS" value="POT-LIN-BOURNS"/>
<element name="R29" library="resistor" package="0207/12" value="0"/>
<element name="P16" library="perso" package="POT-LIN-BOURNS" value="POT-LIN-BOURNS"/>
<element name="PL1" library="con-harting-v" package="40V" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="ACO1" library="con-phoenix-254" package="2POL254" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="ACO2" library="con-phoenix-254" package="2POL254" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="ACI1" library="con-phoenix-254" package="2POL254" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="ACI2" library="con-phoenix-254" package="2POL254" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="PL2" library="con-harting-v" package="40V" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="B1" library="con-phoenix-254" package="2POL254" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="B2" library="con-phoenix-254" package="2POL254" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="B3" library="con-phoenix-254" package="2POL254" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="B4" library="con-phoenix-254" package="2POL254" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="B5" library="con-phoenix-254" package="2POL254" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="B6" library="con-phoenix-254" package="2POL254" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="B7" library="con-phoenix-254" package="2POL254" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="B8" library="con-phoenix-254" package="2POL254" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="B9" library="con-phoenix-254" package="2POL254" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="B10" library="con-phoenix-254" package="2POL254" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="B11" library="con-phoenix-254" package="2POL254" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="B12" library="con-phoenix-254" package="2POL254" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="B13" library="con-phoenix-254" package="2POL254" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="B14" library="con-phoenix-254" package="2POL254" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="B15" library="con-phoenix-254" package="2POL254" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="B16" library="con-phoenix-254" package="2POL254" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="CLE" library="con-phoenix-254" package="3POL254" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="JPBP" library="con-phoenix-254" package="3POL254" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
</elements>
<signals>
<signal name="N$2">
<contactref element="D3" pad="C"/>
<contactref element="D4" pad="A"/>
<contactref element="ACI1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="D2" pad="C"/>
<contactref element="D4" pad="C"/>
<contactref element="C1" pad="+"/>
<contactref element="IC3" pad="IN"/>
</signal>
<signal name="N$6">
<contactref element="R1" pad="2"/>
<contactref element="OK1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="6"/>
<contactref element="R3" pad="2"/>
<contactref element="DMX-T" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="7"/>
<contactref element="R3" pad="1"/>
<contactref element="DMX-T" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="R1" pad="1"/>
<contactref element="IC4" pad="26"/>
</signal>
<signal name="N$13">
<contactref element="IC2" pad="6"/>
<contactref element="R4" pad="2"/>
<contactref element="DMX-R" pad="3"/>
</signal>
<signal name="N$14">
<contactref element="IC2" pad="7"/>
<contactref element="R4" pad="1"/>
<contactref element="DMX-R" pad="2"/>
</signal>
<signal name="GND">
<contactref element="OK1" pad="5"/>
<contactref element="IC1" pad="5"/>
<contactref element="DMX-T" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="D3" pad="A"/>
<contactref element="C1" pad="-"/>
<contactref element="IC3" pad="GND"/>
<contactref element="C2" pad="2"/>
<contactref element="IC2" pad="2"/>
<contactref element="IC2" pad="3"/>
<contactref element="IC2" pad="4"/>
<contactref element="OK2" pad="2"/>
<contactref element="IC2" pad="5"/>
<contactref element="DMX-R" pad="1"/>
<contactref element="IC5" pad="5"/>
<contactref element="OK3" pad="5"/>
<contactref element="IC5" pad="5"/>
<contactref element="DMX-T1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="8"/>
<contactref element="IC3" pad="OUT"/>
<contactref element="C2" pad="1"/>
<contactref element="IC2" pad="8"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="OK1" pad="8"/>
<contactref element="IC5" pad="8"/>
<contactref element="IC5" pad="8"/>
<contactref element="IC5" pad="3"/>
<contactref element="IC5" pad="2"/>
<contactref element="R22" pad="2"/>
<contactref element="OK3" pad="8"/>
</signal>
<signal name="N$4">
<contactref element="R5" pad="2"/>
<contactref element="OK2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="IC2" pad="1"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$32">
<contactref element="OK2" pad="7"/>
<contactref element="R6" pad="1"/>
<contactref element="IC4" pad="25"/>
</signal>
<signal name="N$15">
<contactref element="OK2" pad="8"/>
<contactref element="R6" pad="2"/>
<contactref element="IC4" pad="3"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$97">
<contactref element="IC1" pad="4"/>
<contactref element="R2" pad="1"/>
<contactref element="OK1" pad="7"/>
</signal>
<signal name="N$40">
<contactref element="IC4" pad="4"/>
</signal>
<signal name="N$101">
<contactref element="D7" pad="C"/>
<contactref element="D8" pad="A"/>
<contactref element="ACI2" pad="1"/>
</signal>
<signal name="N$102">
<contactref element="D6" pad="C"/>
<contactref element="D8" pad="C"/>
<contactref element="C3" pad="+"/>
<contactref element="IC4" pad="6"/>
</signal>
<signal name="GND1">
<contactref element="D5" pad="A"/>
<contactref element="D7" pad="A"/>
<contactref element="C3" pad="-"/>
<contactref element="OK2" pad="5"/>
<contactref element="OK1" pad="2"/>
<contactref element="IC4" pad="5"/>
<contactref element="OK3" pad="2"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$104">
<contactref element="R21" pad="2"/>
<contactref element="OK3" pad="1"/>
</signal>
<signal name="N$105">
<contactref element="IC5" pad="6"/>
<contactref element="R23" pad="2"/>
<contactref element="DMX-T1" pad="3"/>
</signal>
<signal name="N$106">
<contactref element="IC5" pad="7"/>
<contactref element="R23" pad="1"/>
<contactref element="DMX-T1" pad="2"/>
</signal>
<signal name="N$107">
<contactref element="R21" pad="1"/>
<contactref element="IC4" pad="28"/>
</signal>
<signal name="N$108">
<contactref element="IC5" pad="4"/>
<contactref element="R22" pad="1"/>
<contactref element="OK3" pad="7"/>
</signal>
<signal name="N$110">
<contactref element="F1" pad="2"/>
<contactref element="TR1" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="AC-1" pad="1"/>
<contactref element="F1" pad="1"/>
</signal>
<signal name="N$103">
<contactref element="AC-1" pad="2"/>
<contactref element="TR1" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="R7" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$8">
<contactref element="R8" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="R9" pad="1"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$16">
<contactref element="IC4" pad="36"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="IC4" pad="33"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="IC4" pad="34"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="IC4" pad="45"/>
</signal>
<signal name="N$20">
<contactref element="IC4" pad="81"/>
<contactref element="P9" pad="P$2"/>
<contactref element="P16" pad="P$2"/>
<contactref element="P15" pad="P$2"/>
<contactref element="P14" pad="P$2"/>
<contactref element="P13" pad="P$2"/>
<contactref element="P12" pad="P$2"/>
<contactref element="P11" pad="P$2"/>
<contactref element="P10" pad="P$2"/>
<contactref element="P1" pad="P$2"/>
<contactref element="P8" pad="P$2"/>
<contactref element="P7" pad="P$2"/>
<contactref element="P6" pad="P$2"/>
<contactref element="P5" pad="P$2"/>
<contactref element="P4" pad="P$2"/>
<contactref element="P3" pad="P$2"/>
<contactref element="P2" pad="P$2"/>
<contactref element="IC4" pad="82"/>
<contactref element="PL1" pad="39"/>
<contactref element="PL1" pad="40"/>
<contactref element="LED1" pad="K"/>
<contactref element="LED3" pad="K"/>
<contactref element="LED2" pad="K"/>
</signal>
<signal name="N$22">
<contactref element="IC4" pad="47"/>
<contactref element="IC4" pad="48"/>
<contactref element="P9" pad="P$1"/>
<contactref element="P16" pad="P$1"/>
<contactref element="P10" pad="P$1"/>
<contactref element="P11" pad="P$1"/>
<contactref element="P12" pad="P$1"/>
<contactref element="P13" pad="P$1"/>
<contactref element="P14" pad="P$1"/>
<contactref element="P15" pad="P$1"/>
<contactref element="P1" pad="P$1"/>
<contactref element="P8" pad="P$1"/>
<contactref element="P2" pad="P$1"/>
<contactref element="P3" pad="P$1"/>
<contactref element="P4" pad="P$1"/>
<contactref element="P5" pad="P$1"/>
<contactref element="P6" pad="P$1"/>
<contactref element="P7" pad="P$1"/>
<contactref element="PL1" pad="1"/>
<contactref element="PL1" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="IC4" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="C4" pad="2"/>
<contactref element="X1" pad="2"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="X1" pad="1"/>
<contactref element="IC4" pad="1"/>
</signal>
<signal name="ADC8">
<contactref element="IC4" pad="15"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="ADC9">
<contactref element="IC4" pad="16"/>
<contactref element="R20" pad="1"/>
</signal>
<signal name="ADC10">
<contactref element="IC4" pad="17"/>
<contactref element="R24" pad="1"/>
</signal>
<signal name="ADC11">
<contactref element="IC4" pad="18"/>
<contactref element="R25" pad="1"/>
</signal>
<signal name="ADC12">
<contactref element="IC4" pad="19"/>
<contactref element="R26" pad="1"/>
</signal>
<signal name="ADC13">
<contactref element="IC4" pad="20"/>
<contactref element="R27" pad="1"/>
</signal>
<signal name="ADC14">
<contactref element="IC4" pad="21"/>
<contactref element="R28" pad="1"/>
</signal>
<signal name="ADC15">
<contactref element="IC4" pad="22"/>
<contactref element="R29" pad="1"/>
</signal>
<signal name="ADC0">
<contactref element="IC4" pad="7"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="ADC1">
<contactref element="IC4" pad="8"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="ADC2">
<contactref element="IC4" pad="9"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="ADC3">
<contactref element="IC4" pad="10"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="ADC4">
<contactref element="IC4" pad="11"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="ADC5">
<contactref element="IC4" pad="12"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="ADC6">
<contactref element="IC4" pad="13"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="ADC7">
<contactref element="IC4" pad="14"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="PA0">
<contactref element="IC4" pad="49"/>
<contactref element="PL1" pad="3"/>
</signal>
<signal name="PA1">
<contactref element="IC4" pad="50"/>
<contactref element="PL1" pad="4"/>
</signal>
<signal name="PA2">
<contactref element="IC4" pad="51"/>
<contactref element="PL1" pad="5"/>
</signal>
<signal name="PA3">
<contactref element="IC4" pad="52"/>
<contactref element="PL1" pad="6"/>
</signal>
<signal name="PA4">
<contactref element="IC4" pad="53"/>
<contactref element="PL1" pad="7"/>
</signal>
<signal name="PA5">
<contactref element="IC4" pad="54"/>
<contactref element="PL1" pad="8"/>
</signal>
<signal name="PA6">
<contactref element="IC4" pad="55"/>
<contactref element="PL1" pad="9"/>
</signal>
<signal name="PA7">
<contactref element="IC4" pad="56"/>
<contactref element="PL1" pad="10"/>
</signal>
<signal name="PC0">
<contactref element="IC4" pad="64"/>
<contactref element="PL1" pad="18"/>
</signal>
<signal name="PC1">
<contactref element="IC4" pad="63"/>
<contactref element="PL1" pad="17"/>
</signal>
<signal name="PC2">
<contactref element="IC4" pad="62"/>
<contactref element="PL1" pad="16"/>
</signal>
<signal name="PC3">
<contactref element="IC4" pad="61"/>
<contactref element="PL1" pad="15"/>
</signal>
<signal name="PC4">
<contactref element="IC4" pad="60"/>
<contactref element="PL1" pad="14"/>
</signal>
<signal name="PC5">
<contactref element="IC4" pad="59"/>
<contactref element="PL1" pad="13"/>
</signal>
<signal name="PC6">
<contactref element="IC4" pad="58"/>
<contactref element="PL1" pad="12"/>
</signal>
<signal name="PC7">
<contactref element="IC4" pad="57"/>
<contactref element="PL1" pad="11"/>
</signal>
<signal name="N$21">
<contactref element="D5" pad="C"/>
<contactref element="D6" pad="A"/>
<contactref element="ACI2" pad="2"/>
</signal>
<signal name="N$28">
<contactref element="D1" pad="C"/>
<contactref element="D2" pad="A"/>
<contactref element="ACI1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="TR1" pad="6"/>
<contactref element="ACO1" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="TR1" pad="5"/>
<contactref element="ACO1" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="TR1" pad="4"/>
<contactref element="ACO2" pad="1"/>
</signal>
<signal name="N$33">
<contactref element="TR1" pad="3"/>
<contactref element="ACO2" pad="2"/>
</signal>
<signal name="PD7">
<contactref element="IC4" pad="65"/>
<contactref element="PL1" pad="19"/>
</signal>
<signal name="PG2">
<contactref element="IC4" pad="66"/>
<contactref element="PL1" pad="20"/>
</signal>
<signal name="N$34">
<contactref element="JPBP" pad="3"/>
<contactref element="PL2" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="PL2" pad="39"/>
<contactref element="JPBP" pad="1"/>
</signal>
<signal name="N$36">
<contactref element="JPBP" pad="2"/>
<contactref element="B1" pad="2"/>
<contactref element="B2" pad="2"/>
<contactref element="B3" pad="2"/>
<contactref element="B4" pad="2"/>
<contactref element="B5" pad="2"/>
<contactref element="B6" pad="2"/>
<contactref element="B7" pad="2"/>
<contactref element="B8" pad="2"/>
<contactref element="B9" pad="2"/>
<contactref element="B10" pad="2"/>
<contactref element="B11" pad="2"/>
<contactref element="B12" pad="2"/>
<contactref element="B13" pad="2"/>
<contactref element="B14" pad="2"/>
<contactref element="B15" pad="2"/>
<contactref element="B16" pad="2"/>
<contactref element="CLE" pad="1"/>
</signal>
<signal name="BP10">
<contactref element="B10" pad="1"/>
<contactref element="PL2" pad="17"/>
</signal>
<signal name="N$54">
<contactref element="PL2" pad="19"/>
<contactref element="CLE" pad="3"/>
</signal>
<signal name="N$55">
<contactref element="PL2" pad="20"/>
<contactref element="CLE" pad="2"/>
</signal>
<signal name="BP1">
<contactref element="PL2" pad="3"/>
<contactref element="B1" pad="1"/>
</signal>
<signal name="BP3">
<contactref element="PL2" pad="5"/>
<contactref element="B3" pad="1"/>
</signal>
<signal name="BP5">
<contactref element="PL2" pad="7"/>
<contactref element="B5" pad="1"/>
</signal>
<signal name="BP7">
<contactref element="PL2" pad="9"/>
<contactref element="B7" pad="1"/>
</signal>
<signal name="BP16">
<contactref element="PL2" pad="11"/>
<contactref element="B16" pad="1"/>
</signal>
<signal name="BP14">
<contactref element="PL2" pad="13"/>
<contactref element="B14" pad="1"/>
</signal>
<signal name="BP12">
<contactref element="PL2" pad="15"/>
<contactref element="B12" pad="1"/>
</signal>
<signal name="BP2">
<contactref element="PL2" pad="4"/>
<contactref element="B2" pad="1"/>
</signal>
<signal name="BP4">
<contactref element="PL2" pad="6"/>
<contactref element="B4" pad="1"/>
</signal>
<signal name="BP6">
<contactref element="PL2" pad="8"/>
<contactref element="B6" pad="1"/>
</signal>
<signal name="BP8">
<contactref element="PL2" pad="10"/>
<contactref element="B8" pad="1"/>
</signal>
<signal name="BP15">
<contactref element="PL2" pad="12"/>
<contactref element="B15" pad="1"/>
</signal>
<signal name="BP13">
<contactref element="PL2" pad="14"/>
<contactref element="B13" pad="1"/>
</signal>
<signal name="BP11">
<contactref element="PL2" pad="16"/>
<contactref element="B11" pad="1"/>
</signal>
<signal name="BP9">
<contactref element="PL2" pad="18"/>
<contactref element="B9" pad="1"/>
</signal>
<signal name="PG1">
<contactref element="PL1" pad="21"/>
<contactref element="IC4" pad="67"/>
</signal>
<signal name="PG0">
<contactref element="PL1" pad="22"/>
<contactref element="IC4" pad="68"/>
</signal>
<signal name="PL7">
<contactref element="PL1" pad="23"/>
<contactref element="IC4" pad="69"/>
</signal>
<signal name="PL5">
<contactref element="PL1" pad="25"/>
<contactref element="IC4" pad="71"/>
</signal>
<signal name="PL3">
<contactref element="PL1" pad="27"/>
<contactref element="IC4" pad="73"/>
</signal>
<signal name="PL1">
<contactref element="PL1" pad="29"/>
<contactref element="IC4" pad="75"/>
</signal>
<signal name="PL6">
<contactref element="PL1" pad="24"/>
<contactref element="IC4" pad="70"/>
</signal>
<signal name="PL4">
<contactref element="PL1" pad="26"/>
<contactref element="IC4" pad="72"/>
</signal>
<signal name="PL2">
<contactref element="PL1" pad="28"/>
<contactref element="IC4" pad="74"/>
</signal>
<signal name="PL0">
<contactref element="PL1" pad="30"/>
<contactref element="IC4" pad="76"/>
</signal>
<signal name="PB1">
<contactref element="PL1" pad="33"/>
<contactref element="IC4" pad="79"/>
</signal>
<signal name="PB2">
<contactref element="PL1" pad="32"/>
<contactref element="IC4" pad="78"/>
</signal>
<signal name="PB0">
<contactref element="PL1" pad="34"/>
<contactref element="IC4" pad="80"/>
</signal>
<signal name="PB3">
<contactref element="IC4" pad="77"/>
<contactref element="PL1" pad="31"/>
</signal>
<signal name="N$26">
<contactref element="R19" pad="2"/>
<contactref element="P9" pad="CURS"/>
</signal>
<signal name="N$31">
<contactref element="R11" pad="2"/>
<contactref element="P1" pad="CURS"/>
</signal>
<signal name="N$37">
<contactref element="R20" pad="2"/>
<contactref element="P10" pad="CURS"/>
</signal>
<signal name="N$38">
<contactref element="R24" pad="2"/>
<contactref element="P11" pad="CURS"/>
</signal>
<signal name="N$39">
<contactref element="R25" pad="2"/>
<contactref element="P12" pad="CURS"/>
</signal>
<signal name="N$41">
<contactref element="R26" pad="2"/>
<contactref element="P13" pad="CURS"/>
</signal>
<signal name="N$42">
<contactref element="R27" pad="2"/>
<contactref element="P14" pad="CURS"/>
</signal>
<signal name="N$43">
<contactref element="R28" pad="2"/>
<contactref element="P15" pad="CURS"/>
</signal>
<signal name="N$44">
<contactref element="R29" pad="2"/>
<contactref element="P16" pad="CURS"/>
</signal>
<signal name="N$45">
<contactref element="R18" pad="2"/>
<contactref element="P8" pad="CURS"/>
</signal>
<signal name="N$46">
<contactref element="R17" pad="2"/>
<contactref element="P7" pad="CURS"/>
</signal>
<signal name="N$47">
<contactref element="R16" pad="2"/>
<contactref element="P6" pad="CURS"/>
</signal>
<signal name="N$48">
<contactref element="R15" pad="2"/>
<contactref element="P5" pad="CURS"/>
</signal>
<signal name="N$49">
<contactref element="R14" pad="2"/>
<contactref element="P4" pad="CURS"/>
</signal>
<signal name="N$50">
<contactref element="R13" pad="2"/>
<contactref element="P3" pad="CURS"/>
</signal>
<signal name="N$51">
<contactref element="R12" pad="2"/>
<contactref element="P2" pad="CURS"/>
</signal>
<signal name="N$52">
</signal>
<signal name="N$53">
</signal>
<signal name="N$56">
</signal>
</signals>
</board>
</drawing>
</eagle>
